General Specifications

1. Work will be completed within stipulated schedule time according to design & Specification.
2. The work should be completed, strictly following the approved Drawing.
3. Before starting of the work a Model section will be constructed by contractor. After checking of Model section as per design & Specification by concerned BWDB Officer Work should be commended.
4. The quantity of item described in bill of quantities may increase of decrease as per field condition.
5. Before starting of work, pre work survey will be done by concerned BWDB Officers, Taskforce Member, BWDB.
6. The contractor /Authorized representative should sign the pre work level book.
7. The number of lead in earthwork provided in estimate may very as per field condition.
8. Final Measurement will be given by Taskforce Committee, BWDB for CC blocks, Earth volume and Go-bags.